
[GENERAL]
Rules=0                         
GarageDisplayFlags=7            
Mass=570.0                      
Inertia=(820.0, 1255.0, 281.0)   
FuelTankPos=(0.00, 0.15, -1.45) 
FuelTankMotion=(560.0,0.7)      
Notes=""
Symmetric=1
DamageFile=F5000_damage           
CGHeight=0.205                  
CGRightRange=(0.500, 0.005, 0)  
CGRightSetting=0
CGRearRange=(0.56, 0.005, 0)    
CGRearSetting=0
GraphicalOffset=(0.0, 0.04, 0.0) 
Undertray00=(0.20,  0.0, -1.00) 
Undertray01=(-0.20, 0.0, -1.00) 
Undertray02=(0.20,  0.0, 1.30)  
Undertray03=(-0.20, 0.0, 1.30)  
Undertray04=(0.58, 0.025, -0.50)
Undertray05=(-0.58, 0.025, -0.50)
Undertray06=(0.58, 0.025, 0.80)
Undertray07=(-0.58, 0.025, 0.80)
Undertray08=(0.58, 0.025, 0.0)
Undertray09=(0.0, 0.0, 0.0)
Undertray10=(-0.58, 0.025, 0.0)
UndertrayParams=(100000, 5000, 1.6) 
TireBrand=F5000_Firestone
FrontTireCompoundSetting=1      
RearTireCompoundSetting=1 
FuelRange=(1.0, 1.0, 120)
FuelSetting=29
NumPitstopsRange=(0, 1, 2)
NumPitstopsSetting=1
Pitstop1Range=(1.0, 1.0, 45)
Pitstop1Setting=0
AIAimSpeedsPerWP=(25.0, 32.0, 40.0, 55.0, 75.0, 95.0, 115.0, 200.0)
AICornerReductionBase=180.0
AIMinPassesPerTick=3            
AIRotationThreshold=0.15        
AIEvenSuspension=0.0            
AISpringRate=1.0                
AIDamperSlow=0.5                
AIDamperFast=0.5                
AIDownforceZArm=-0.100          
AIDownforceBias=0.5             
AITorqueStab=(1.0, 1.0, 1.0)    
AIPerfUsage=(0.85, 1.0, 0.95)
FeelerFlags=15                   
FeelerOffset=(0.0, 0.0, 0.0)    
FeelersAtCGHeight=1 
FeelerFrontLeft=(1.00,0.250,-1.670)      
FeelerFrontRight=(-1.00,0.250,-1.670)   
FeelerRearLeft=(1.10,0.30,1.73)       
FeelerRearRight=(-1.10,0.30,1.73)    
FeelerFront=(0.0,0.06,-2.17)            
FeelerRear=(0.0,0.20,1.87)              
FeelerRight=(-0.72,0.36,-0.00)        
FeelerLeft=(0.72,0.36,-0.00)          
FeelerTopFrontLeft=(-0.0,0.06,0.87)  
FeelerTopFrontRight=(0.0,0.06,0.87) 
FeelerTopRearLeft=(-0.56,0.85,2.04) 
FeelerTopRearRight=(0.56,0.85,2.04)   
FeelerBottom=(0.0,0.70,0.00)  

[PITMENU]
StopGo=1                          
Fuel=1                              
AllTires=1                          
FrontRearTires=(0,0)                
LeftRightTires=(0,0)                
IndividualTires=(0,0,0,0)           
FenderFlare=(0,0)                   
FrontWing=0                         
RearWing=0                          
Driver=0                            
Wedge=0                             
Radiator=0                          
TrackBar=0                          
Pressure=(0,0,0,0)                  
SpringRubber=(0,0,0,0)              
Damage=1                            
StopGoSimultaneous=0                
PressureOnTheFly=0                  
DamagedTiresOnly=0                  
CompoundRestrictions=0              
Preparation=(100.0,40.0,0.5,4.5)    
TireTime=(12.5,25.0,3.5,0.0) 
FuelTime=(1.0,1.0,1.0,0.5,0.0)         
FrontWingTime=(8.0,25.0)            
RearWingTime=(12.0,30.0)            
DamageTime=(30.0,8.0,720.0,1.0)        

[AIDPENALTIES] 
TC=(0.00,0.005,0.010)               
ABS=(0.000,0.005,0.010)            
Stability=(0.000,0.005,0.010)       
Autoshift=(0.00,0.005,0.005,0.010)     
Steering=(0.000,0.005,0.008,0.020)  
Braking=(0.005,0.010,0.015)
Invulnerable=(0.00,0.00)            
Opposite=(0.00,0.005)                
SpinRecovery=(0.00,0.005)            
AutoPit=(0.00,0.005)                 
AutoLift=(0.00,0.005)                
AutoBlip=(0.00,0.005)      
   
[FRONTWING]
FWRange=(1.0, 1.0, 5)          
FWSetting=1                     
FWDragParams=(0.030, 0.00535, 0.00001)        
FWLiftParams=(-0.1432, -0.030, 0.00) // 
FWLiftSideways=(0.25)      
FWLiftPeakYaw=(0.0, 1.0)    
FWLeft=(-0.04, 0.0, 0.0)       
FWRight=(0.04, 0.0, 0.0)     
FWUp=(0.0, -0.09, 0.009)     
FWDown=(0.0, 0.09,-0.005)     
FWAft=(0.0, 0.04, -0.04)   
FWFore=(0.0, 0.0, 0.0)         
FWRot=(0.10, 0.05, 0.15)       
FWCenter=(0.00, -0.00, -0.50)   

[REARWING]
RWRange=(1.0, 1.0, 6)        
RWSetting=2           
RWDragParams=(0.0510, 0.01759, 0.00002)       
RWLiftParams=(-0.1399, -0.03, 0.00) //
RWLiftSideways=(0.25)         
RWLiftPeakYaw=(0.0, 1.0)      
RWLeft=(-0.07, 0.0, 0.0)      
RWRight=(0.07, 0.0, 0.0)       
RWUp=(0.0, -0.12, 0.04)      
RWDown=(0.0, 0.12,-0.02)    
RWAft=(0.0, 0.08, -0.08)       
RWFore=(0.0, 0.0, 0.0)        
RWRot=(0.10, 0.05, 0.15)      
RWCenter=(0.00, 0.65, 0.45)      

[BODYAERO]
BodyDragBase=(0.2850)          
BodyDragHeightAvg=(0.350)     
BodyDragHeightDiff=(0.900)     
BodyMaxHeight=(0.40)          
BodyLeft=(-0.7, 0.0, 0.0)       
BodyRight=(0.7, 0.0, 0.0)    
BodyUp=(0.0, -1.7, 0.0)      
BodyDown=(0.0, 1.7, 0.0)     
BodyAft=(0.0, 0.10, -1.00)    
BodyFore=(0.0, -0.2200, 0.370)  
BodyRot=(4.0, 3.0, 2.0)     
BodyCenter=(0.0, 0.290, -1.310) 
RadiatorRange=(0.0, 2.0, 2)    
RadiatorSetting=2               
RadiatorDrag=(0.0162)        
RadiatorLift=(0.0103)      
BrakeDuctRange=(0.0, 1.0, 4)    
BrakeDuctSetting=2          
BrakeDuctDrag=(0.0050)        
BrakeDuctLift=(0.0110)          

[SUSPENSION]
PhysicalModelFile=TS11_Susp.pm
CorrectedInnerSuspHeight=0.240    	//0.240
ApplySlowToFastDampers=1         
AdjustSuspRates=1                
AlignWheels=1				//1                    
FrontWheelTrack=0         		//// If non-zero, forces the front wheels to be specified track width  FrontWheelTrack=1.660
RearWheelTrack=0         		//RearWheelTrack=1.570  
LeftWheelBase=0  			//LeftWheelBase=2.74000           
RightWheelBase=0 			//RightWheelBase=2.74000               
SpringBasedAntiSway=1            
AllowNoAntiSway=1                
FrontAntiSwayBase=0.0
FrontAntiSwayRange=(10000.0, 10000.0, 9)
FrontAntiSwaySetting=5
FrontAntiSwayRate=(1.00e11, 4.0) 
RearAntiSwayBase=0.0
RearAntiSwayRange=(10000.0, 10000.0, 9)
RearAntiSwaySetting=2
RearAntiSwayRate=(1.00e11, 4.0)  
FrontToeInRange=(-1.0, 0.05, 41)
FrontToeInSetting=17
RearToeInRange=(-1.0, 0.05, 41)
RearToeInSetting=21
LeftCasterRange=(-2.0, 0.1, 81)       
LeftCasterSetting=45
RightCasterRange=(-2.0, 0.1, 81)      
RightCasterSetting=45

[CONTROLS]
SteeringFFBMult=4.0
SteerLockRange=(5.0, 1.0, 25)
SteerLockSetting=11
RearBrakeRange=(0.250, 0.005, 101)
RearBrakeSetting=40
BrakePressureRange=(0.80, 0.02, 11)
BrakePressureSetting=5
HandbrakePressRange=(0.00, 0.05, 1) 
HandbrakePressSetting=0
//UpshiftAlgorithm=(0.975,0.0)        
//DownshiftAlgorithm=(0.91,0.70,0.60) 
AutoUpshiftGripThresh=0.65         
AutoDownshiftGripThresh=0.60        
TractionControlGrip=(1.00, 0.20)    
TractionControlLevel=(0.35, 0.95)   
ABS4Wheel=1                         
ABSGrip=(1.00, 0.20)                
ABSLevel=(0.40, 0.95)               
OnboardBrakeBias=0                  

[ENGINE]
SpeedLimiter=0                      
Normal=1972_Chevy_Morand_Engine                  
RestrictorPlate=1972_Chevy_Morand_Engine    

[DRIVELINE]
ClutchEngageRate=0.6                
ClutchInertia=0.01312              
ClutchTorque=1971.0                  
ClutchWear=0.1                      
ClutchFriction=9.10                 
BaulkTorque=690.0                   
AllowManualOverride=1               
SemiAutomatic=0                     
UpshiftDelay=0.28                  
UpshiftClutchTime=0.28             
UpshiftLiftThrottle=0.00           
DownshiftDelay=0.28                
DownshiftClutchTime=0.25           
DownshiftBlipThrottle=0.65            
WheelDrive=REAR 
GearFile=Chevy_gears.ini                 
FinalDriveSetting=4                 
ForwardGears=5
ReverseSetting=3
Gear1Setting=8
Gear2Setting=18
Gear3Setting=28
Gear4Setting=37
Gear5Setting=44
DiffPowerRange=(0.0,0.05,21)         
DiffPowerSetting=5                  
DiffCoastRange=(0.0,0.05,21)         
DiffCoastSetting=5                  
DiffPreloadRange=(5.0, 5.0, 5)     
DiffPreloadSetting=0               

[FRONTLEFT]
BumpTravel=-0.015
ReboundTravel=-0.175
BumpStopSpring=12500.0
BumpStopRisingSpring=6.50e6
BumpStopDamper=2763.5
BumpStopRisingDamper=6.00e5
BumpStage2=0.95
ReboundStage2=-0.95
FrictionTorque=1.50
SpinInertia=0.750
CGOffsetX=0.000
PushrodSpindle=(-0.050, -0.150, 0.000)
PushrodBody=(-0.280, 0.170, 0.0)
CamberRange=(-3.5, 0.1, 81)
CamberSetting=5
PressureRange=(90.0, 1.0, 106)
PressureSetting=20
PackerRange=(0.000, 0.001, 41)
PackerSetting=5
SpringMult=0.8                      
SpringRange=(20000.0, 10000.0, 8)
SpringSetting=4
RideHeightRange=(0.040, 0.001, 41)
RideHeightSetting=4
SlowBumpRange=(1300.0, 470.0, 11)
SlowBumpSetting=4
FastBumpRange=(100.0, 490.0, 11)
FastBumpSetting=4
SlowReboundRange=(1800.0, 550.0, 11)
SlowReboundSetting=4
FastReboundRange=(300.0, 490.0, 11)
FastReboundSetting=4
BrakeDiscRange=(0.028, 0.000, 1)    // disc thickness
BrakeDiscSetting=1
BrakePadRange=(0, 0, 1)             // pad type (not implemented)
BrakePadSetting=2
BrakeDiscInertia=0.715              // inertia per meter of thickness
BrakeOptimumTemp=500.0              // optimum brake temperature in Celsius (peak brake grip)
BrakeFadeRange=750.0                // temperature outside of optimum that brake grip drops to half (too hot or too cold)
BrakeWearRate=4.822e-011            // meters of wear per second at optimum temperature
BrakeFailure=(1.43e-002,5.40e-004)  // average and variation in disc thickness at failure
BrakeTorque=1900.0                  // maximum brake torque at zero wear and optimum temp
BrakeHeating=9.500e-004             // heat added linearly with brake torque times wheel speed (at max disc thickness)
BrakeCooling=(1.745e-002,2.334e-004)// minimum brake cooling rate (base and per unit velocity) (at max disc thickness)
BrakeDuctCooling=0.633e-004 

[FRONTRIGHT]
BumpTravel=-0.015
ReboundTravel=-0.175
BumpStopSpring=12500.0
BumpStopRisingSpring=6.50e6
BumpStopDamper=2763.5
BumpStopRisingDamper=6.00e5
BumpStage2=0.95
ReboundStage2=-0.95
FrictionTorque=1.50
SpinInertia=0.750
CGOffsetX=0.000
PushrodSpindle=(0.050, -0.150, 0.000)
PushrodBody=(0.280, 0.170, 0.0)
CamberRange=(-3.5, 0.1, 81)
CamberSetting=5
PressureRange=(90.0, 1.0, 106)
PressureSetting=20
PackerRange=(0.000, 0.001, 41)
PackerSetting=5
SpringMult=0.8                      
SpringRange=(20000.0, 10000.0, 8)
SpringSetting=4
RideHeightRange=(0.040, 0.001, 41)
RideHeightSetting=4
SlowBumpRange=(1300.0, 470.0, 11)
SlowBumpSetting=4
FastBumpRange=(100.0, 490.0, 11)
FastBumpSetting=4
SlowReboundRange=(1800.0, 550.0, 11)
SlowReboundSetting=4
FastReboundRange=(300.0, 490.0, 11)
FastReboundSetting=4
BrakeDiscRange=(0.028, 0.000, 1)    // disc thickness
BrakeDiscSetting=1
BrakePadRange=(0, 0, 1)             // pad type (not implemented)
BrakePadSetting=2
BrakeDiscInertia=0.715              // inertia per meter of thickness
BrakeOptimumTemp=500.0              // optimum brake temperature in Celsius (peak brake grip)
BrakeFadeRange=750.0                // temperature outside of optimum that brake grip drops to half (too hot or too cold)
BrakeWearRate=4.822e-011            // meters of wear per second at optimum temperature
BrakeFailure=(1.43e-002,5.40e-004)  // average and variation in disc thickness at failure
BrakeTorque=1900.0                  // maximum brake torque at zero wear and optimum temp
BrakeHeating=9.500e-004             // heat added linearly with brake torque times wheel speed (at max disc thickness)
BrakeCooling=(1.745e-002,2.334e-004)// minimum brake cooling rate (base and per unit velocity) (at max disc thickness)
BrakeDuctCooling=0.633e-004 

[REARLEFT]
BumpTravel=-0.020
ReboundTravel=-0.220
BumpStopSpring=10000.0
BumpStopRisingSpring=6.50e6
BumpStopDamper=2763.5
BumpStopRisingDamper=6.00e5
BumpStage2=0.95
ReboundStage2=-0.95
FrictionTorque=1.50
SpinInertia=0.750
CGOffsetX=0.0
PushrodSpindle=(-0.050, -0.150, 0.000)
PushrodBody=(-0.325, 0.170, 0.0)
CamberRange=(-3.0, 0.1, 81)
CamberSetting=5
SpringMult=0.8 
PressureRange=(90.0, 1.0, 106)
PressureSetting=25
PackerRange=(0.000, 0.001, 61)
PackerSetting=5                    
SpringRange=(20000.0, 10000.0, 8)
SpringSetting=4
RideHeightRange=(0.040, 0.001, 39)
RideHeightSetting=7
SlowBumpRange=(1300.0, 470.0, 11)
SlowBumpSetting=4
FastBumpRange=(100.0, 490.0, 11)
FastBumpSetting=4
SlowReboundRange=(1800.0, 550.0, 11)
SlowReboundSetting=4
FastReboundRange=(300.0, 490.0, 11)
FastReboundSetting=4
BrakeDiscRange=(0.028, 0.00, 1)    // disc thickness (0.021, 0.007, 2)
BrakeDiscSetting=0		    // =0
BrakePadRange=(0, 0, 1)             // pad type (not implemented)  (0, 1, 5) 
BrakePadSetting=2		    // =2
BrakeDiscInertia=0.715              // inertia per meter of thickness
BrakeOptimumTemp=450.0              // optimum brake temperature in Celsius (peak brake grip)
BrakeFadeRange=750.0                // temperature outside of optimum that brake grip drops to half (too hot or too cold)
BrakeWearRate=4.822e-011            // meters of wear per second at optimum temperature
BrakeFailure=(1.43e-002,5.40e-004)  // average and variation in disc thickness at failure
BrakeTorque=1400.0                  // maximum brake torque at zero wear and optimum temp
BrakeHeating=9.500e-004             // heat added linearly with brake torque times wheel speed (at max disc thickness)
BrakeCooling=(1.745e-002,2.334e-004)// minimum brake cooling rate (base and per unit velocity) (at max disc thickness)
BrakeDuctCooling=0.633e-004

[REARRIGHT]
BumpTravel=-0.020
ReboundTravel=-0.220
BumpStopSpring=10000.0
BumpStopRisingSpring=6.50e6
BumpStopDamper=2763.5
BumpStopRisingDamper=6.00e5
BumpStage2=0.95
ReboundStage2=-0.95
FrictionTorque=1.50
SpinInertia=0.750
CGOffsetX=0.0
PushrodSpindle=(0.050, -0.150, 0.000)
PushrodBody=(0.325, 0.170, 0.0)
CamberRange=(-3.0, 0.1, 81)
CamberSetting=5
SpringMult=0.8 
PressureRange=(90.0, 1.0, 106)
PressureSetting=25
PackerRange=(0.000, 0.001, 61)
PackerSetting=5                    
SpringRange=(20000.0, 10000.0, 8)
SpringSetting=4
RideHeightRange=(0.040, 0.001, 39)
RideHeightSetting=7
SlowBumpRange=(1300.0, 470.0, 11)
SlowBumpSetting=4
FastBumpRange=(100.0, 490.0, 11)
FastBumpSetting=4
SlowReboundRange=(1800.0, 550.0, 11)
SlowReboundSetting=4
FastReboundRange=(300.0, 490.0, 11)
FastReboundSetting=4
BrakeDiscRange=(0.028, 0.00, 1)    // disc thickness (0.021, 0.007, 2)
BrakeDiscSetting=0		    // =0
BrakePadRange=(0, 0, 1)             // pad type (not implemented)  (0, 1, 5) 
BrakePadSetting=2		    // =2
BrakeDiscInertia=0.715              // inertia per meter of thickness
BrakeOptimumTemp=450.0              // optimum brake temperature in Celsius (peak brake grip)
BrakeFadeRange=750.0                // temperature outside of optimum that brake grip drops to half (too hot or too cold)
BrakeWearRate=4.822e-011            // meters of wear per second at optimum temperature
BrakeFailure=(1.43e-002,5.40e-004)  // average and variation in disc thickness at failure
BrakeTorque=1400.0                  // maximum brake torque at zero wear and optimum temp
BrakeHeating=9.500e-004             // heat added linearly with brake torque times wheel speed (at max disc thickness)
BrakeCooling=(1.745e-002,2.334e-004)// minimum brake cooling rate (base and per unit velocity) (at max disc thickness)
BrakeDuctCooling=0.633e-004



